**Category C9 - Kart Junior- 6 - 15 Years**

**1. Definition**

A: The C9 category allows vehicles whose chassis / frames come from karts with engines or are approved by the ***Fédération internationale de Speeddown*** and comply with the provisions of these regulations. The karts must have a rigid axle and no ballast is permitted.

B: Copies of individual parts are not permitted. There are only components from registered companies which on the one hand are liable for their products and on the other hand offer complete vehicles and/or their individual parts on the market for everyone.

**2. Dimensions**

No changes may be made to the chassis / frames.

|  |  |  |
| --- | --- | --- |
| **wheelbase** | Max. 1100 mm | |
| **width (front)** | Max. 1200 mm | |
| **width (rear)** | Max. 1400 mm | |
| **chassis clearance** | Min. 20 mm | Max. 80 mm |
| **rims** | 5 ‘’ | |
| **bearings (front)** | inside-Ø min 17 mm | |
| **bearings (rear)** | inside-Ø min 25 mm | |
| **tire (front)** | Min 10 x 4.00-5  Ma. 10 x 4.50-5 | |
| **tire (rear)** | Min 11 x 5.00-5  Max 11 x 7.10-5 | |

**3. Weight**

The **maximum permissible empty weight of the vehicle** is **65 kg** and is also defined in the general vehicle construction regulations.

If the empty weight is exceeded, the driver will be classified and evaluated in category C8.

**4. Ballast**

Ballast must be secured to the chassis (at least M8).

Ballast may also be secured to the base plate using screws (at least M8) and large washers.

The use of ballast in the chassis structure is not permitted.

**5. Chassis / Frames**

The frame must be made of tubular steel and must not be modified. Fibre-reinforced plastic material and light metals are not allowed. No sharp edges or pointed ends are permitted. All individual parts of the frame must be firmly connected to one another.

All drive elements must be removed. (motor, pinion, etc.). The tank may be used as storage space.

The use of suspension elements, complete suspension or similar systems are not permitted.

The tube bumpers (front and rear) and the brackets for the bodywork must be firmly connected to the frame (Screw or quick fastener). The recommended dimensions correspond to the standardized specifications of the kart manufacturers, these are Ø 16mm at the front and Ø 20mm at the rear.

A one-piece magnetic steel base plate must be firmly screwed to the frames between the outer frame tubes. The base plate must not protrude beyond the outer frame tubes. The kart floor must consist of sheet metal (steel) with a minimum thickness of 1.5 mm.Welded joints are not permitted. The floor plate must at least completely cover the area between the cross tube in front of the seat and the front tube, as well as the outer frame tubes. A continuous floor plate between the front and rear tubes is permitted.

**6. Steering**

The steering must be built in a typical kart style. This consists of a steering column, fixed and metallic steering rods and must be operated with a steering wheel. All screwed steering elements must be secured with lock nuts.

**7. Bodywork**

Front spoilers, front fairing and side boxes that have been homologated by the CIK / FIA must be installed. Even after the CIK / FIA homologation has expired, they can be used for speeddown races.

The outside of the sidepods must be in line with the outside of the rear wheel. **The deviation may not exceed ±2 cm.** This rule does not apply to fitted rain tires.

A tubular steel or plastic rear bumper must be attached to the frame. Plastic bumpers must be homologated by the CIK / FIA. Even after the CIK / FIA homologation has expired, the rear bumper can be used for speeddown races.

**8. Seat**

Only seats from motor karting are permitted. The kart seat must keep the driver in a fixed position throughout the race run. Kart seats with headrests are only allowed if they are homologated according to CIK/FIA (Test Specification for Karting High Seats). The homologation is still valid after the CIK/FIA approval for speeddown races has expired.

**9. Tires**

Only tires from motor karting are permitted. Except for normal wear and tear, no changes may be made to the tires. **The air pressure must not exceed 3.0 bar**.

**10. Rear axle**

The rear axle must be in one piece (rigid axle) and made of magnetic steel. Solid axles must not be less than 25 mm in diameter and hollow axles of 30 mm over the entire length. 2 ball bearings are sufficient for storage. These are to be attached to the frame with standard bearing shells from motor karting. The rear wheels must be rigidly attached to the rear axle with wheel stars and axle wedges. **Rear wheels mounted independently of the rigid axle are prohibited**.

**11. Brakes**

The brakes on one axle must always act on both wheels. Only foot-operated hydraulic or mechanical disc brakes are permitted. The rear axle must always be braked. The brake disc of the rear rigid axle must be rigidly attached with a mount and axle wedges and have a diameter of at least 150 mm and a material thickness of at least 2 mm. A front brake is also permitted. The power transmission from the brake pedal to the brake cylinder takes place by means of a linkage, which must be additionally secured with a tensioned safety rope made of steel wire. The safety rope must not have any slack. The brake pedal must not protrude beyond the bumper when it is operated.

The pedal and seat position must be adjusted to the driver in such a way that full braking can be carried out in a normal sitting position without the leg being fully stretched during full braking. The brake pedal can be lengthened with pedal attachments or changed in position with adapters attached to the frame.

**12. Lubrication and power units**

Any lubrication and power units are prohibited on the vehicle.

**13. Specific racing equipment**

The provisions of the document “**General FISD Regulations”, Section II, Point B** apply. In addition, wearing a neck brace (as in kart racing) and rib protection are mandatory in this category. Only commercially available products from kart racing are permitted for rib protection (no self-made products).

**14. Start number**

The start number must be attached to the front shield. It must be in accordance with the document **General FISD Regulations Section II, Item I**.

**15. Towing the vehicles**

According to the document **General FISD Regulations Section II, Point F**.

**16. Sanctions**

Failure to comply with these regulations results in the exclusion from the race, without the possibility of special permits in the event of a FISD race.

**17. History - Changes**

First official edition approved on the occasion of the general meeting (GM) in Predappio on November 5th, 2011. Adjustments and approval on the occasion of the GM on November 11, 2012 in Wittinsburg:

* Item 9: No more changes may be made to the tires.

Adjustments and approval on the occasion of the GA on October 25, 2014 in Oberwiesenthal:

* Item 5: Chassis - Attaching protective shields.
* Item 11: Brakes - Brakes at the front are now also permitted.

Adjustments and approval on the occasion of the GA on November 7, 2015 in Stoumont:

* Item 2: Clear definition that no changes to the frame are permitted.
* Item 5: Adaptation of the map definition based on the FIA specifications

Adjustments and approval on the occasion of the GA of November 13, 2016 in Viu:

* Item 8: headrest
* Item 13: Introduction of rib protection

Adjustments and approval on the occasion of the GA vom November 2021 in Freital:

* Structure adapted to C8 regulations.
* Item 1: All chassis/frames derived from karts with engines are allowed (not just "Minime/Cadet/Junior")
* Item 5: deleted - chassis - installation of protective shields.
* The tank may be used as storage space.
* Item 8: Only CIK/FIA homologated kart seats with headrests are allowed.
* Item 9: maximum tire pressure 3.0 bar

Adjustments and approval 2022:

* Item 1: Ballast is allowed
* Item 2: Specification of minimum tire sizes.
* Item 5: Maximum permissible empty weight of the vehicle 65 kg.
* Item 5: One-piece base plate made of magnetic steel with a minimum thickness of 1.5 mm.
* Item 7: When slicks are fitted, the side box must not protrude more than 2 cm over the rear wheel

Amendments approved at the board meeting on November 4, 2024:

* Item 4: Clarification regarding ballast
* Item 5: Steel base plate thickness: 1.5 mm.